**Registering PennPilot Aerials**

1. **Export Registration Table into Registered Images Folder**
2. **Rectify Aerial as a TIFF with JPEG Compression in the Registered Images folder.**
	1. **Projective transformation seems to work well for difficult images.**
	2. **Otherwise 1st order is ok.**
3. **Clip the Raster**
	1. **Check both options**
	2. **Make sure the clip square is selected.**
	3. **Keep the edit session open… things seem to run faster.**
	4. **Output for the Clip goes into the Default GDB by default.**
	5. **Periodically clear the default.gdb and the registered images in the registered images folder… LEAVE THE Registration text files.**
4. **Export the clipped raster as a JPG2000**
	1. **Use Renderer**