Identification_Information:
  Citation:
    Citation_Information:
      Originator: Lancaster County GIS Department
      Publication_Date: 1999
      Title: Lancaster County hydrologic features (less than 10 foot width)
      Geospatial_Data_Presentation_Form: vector digital data
      Publication_Information:
        Publication_Place: Lancaster, PA
        Publisher: Lancaster County GIS Department
      Other_Citation_Details: Created based on 1 inch to 1600 foot aerial photography
      Online_Linkage: http://pasdadev.erri.psu.edu/lanc/lancdownload2.cgi/lancco_hydro_p
  Description:
    Abstract: This coverage stores polygon definitions about hydrologic and drainage features such as lakes, ponds and streams wider than 10 feet.
    Purpose: Data created for Lancaster County planning.  Intended for illustration and demonstration purposes only.
  Time_Period_of_Content:
    Time_Period_Information:
      Single_Date/Time:
        Calendar_Date: 199912
    Currentness_Reference: ground condition
  Status:
    Progress: Complete
    Maintenance_and_Update_Frequency: 5 years
  Spatial_Domain:
    Bounding_Coordinates:
      West_Bounding_Coordinate: -76.734074
      East_Bounding_Coordinate: -75.873641
      North_Bounding_Coordinate: 40.319161
      South_Bounding_Coordinate: 39.716118
  Keywords:
    Theme:
      Theme_Keyword_Thesaurus: none
      Theme_Keyword: hydrology
      Theme_Keyword: lakes
      Theme_Keyword: ponds
      Theme_Keyword: streams
      Theme_Keyword: rivers
      Theme_Keyword: inland waters
    Place:
      Place_Keyword_Thesaurus: none
      Place_Keyword: Lancaster County
      Place_Keyword: Pennsylvania
  Access_Constraints: none
  Use_Constraints:
    For use at 1:2400 or smaller scale.

    For educational/demonstration purposes only.  The Originator, Publisher and Distributor exclude any and all implied warranties and make no warranty or representation with respect to the data files or accompanying documentation, including quality, performance, merchantability or fitness for a particular purpose. These data files and documentation are provided 'as is' and the User assumes the entire risk as to their quality and performance

    These data are not to be redistributed for commercial profit.  Reproduction or redistribution of this digital data set without permission of the Originator/Publisher is expressly forbidden.  The Originator and Publisher should be clearly cited in any product derived from this data.  Any modifications to this data must be described in any digital or hardcopy product derived from this data.
  Point_of_Contact:
    Contact_Information:
      Contact_Person_Primary:
        Contact_Person: Linda McCawley
        Contact_Organization: Lancaster County GIS Department
      Contact_Address:
        Address_Type: mailing and physical address
        Address: 50 North Duke St., PO Box 83480
        City: Lancaster
        State_or_Province: PA
        Postal_Code: 17608-3480
      Contact_Voice_Telephone: 717-391-7550
      Contact_Electronic_Mail_Address: mccawlel@co.lancaster.pa.us
  Native_Data_Set_Environment: Microsoft Windows 2000 Version 5.0 (Build 2195) Service Pack 2; ESRI ArcCatalog 8.1.1.649
  Cross_Reference:
    Citation_Information:
      Originator: Lancaster County GIS Department
      Publication_Date: 1993
      Title: HYDRO - 1993 Lancaster County hydrologic features (less than 10 foot width)
      Publication_Information:
        Publication_Place: Lancaster, PA
        Publisher: Lancaster County GIS Department
      Other_Citation_Details: Created based on 1 inch to 600 foot aerial photography
Data_Quality_Information:
  Attribute_Accuracy:
    Attribute_Accuracy_Report: Verified visually and through field reconnaissance
  Logical_Consistency_Report: Topology exists.
  Completeness_Report: Complete from aerial photography.
  Positional_Accuracy:
    Horizontal_Positional_Accuracy:
      Horizontal_Positional_Accuracy_Report: Accuracy conforms to National Mapping Accuracy Standards of planimetric and topographic mapping data at a design scale of 1"=200'.
  Lineage:
    Source_Information:
      Source_Citation:
        Citation_Information:
          Originator: Aerial Data Reduction Associates, Inc.
          Publication_Date: 1993
          Title: Orthophotographs of Lancaster County - 1993
          Geospatial_Data_Presentation_Form: remote sensing image
      Source_Scale_Denominator: 19200
      Type_of_Source_Media: stable-base material
      Source_Time_Period_of_Content:
        Time_Period_Information:
          Single_Date/Time:
            Calendar_Date: 1993
            Time_of_Day: unknown
        Source_Currentness_Reference: ground condition
      Source_Citation_Abbreviation: aerials
      Source_Contribution: features for digitization
    Process_Step:
      Process_Description: Features digitized from aerial photography.  Supplemented and revised by Lancaster GIS staff from information gathered through assessment, fieldwork and surveys.
      Source_Used_Citation_Abbreviation: aerials
      Process_Date: 1998
  Cloud_Cover: 0
Spatial_Data_Organization_Information:
  Direct_Spatial_Reference_Method: Vector
  Point_and_Vector_Object_Information:
    SDTS_Terms_Description:
      SDTS_Point_and_Vector_Object_Type: G-polygon
      Point_and_Vector_Object_Count: 5000
Spatial_Reference_Information:
  Horizontal_Coordinate_System_Definition:
    Planar:
      Grid_Coordinate_System:
        Grid_Coordinate_System_Name: State Plane Coordinate System 1983
        State_Plane_Coordinate_System:
          SPCS_Zone_Identifier: 3702
          Lambert_Conformal_Conic:
            Standard_Parallel: 39.933333
            Standard_Parallel: 40.966667
            Longitude_of_Central_Meridian: -77.750000
            Latitude_of_Projection_Origin: 39.333333
            False_Easting: 1968500.000000
            False_Northing: 0.000000
      Planar_Coordinate_Information:
        Planar_Coordinate_Encoding_Method: coordinate pair
        Coordinate_Representation:
          Abscissa_Resolution: 0.000512
          Ordinate_Resolution: 0.000512
        Planar_Distance_Units: survey feet
    Geodetic_Model:
      Horizontal_Datum_Name: North American Datum of 1983
      Ellipsoid_Name: Geodetic Reference System 80
      Semi-major_Axis: 6378137.000000
      Denominator_of_Flattening_Ratio: 298.257222
Entity_and_Attribute_Information:
  Detailed_Description:
    Entity_Type:
      Entity_Type_Label: hydro_p
      Entity_Type_Definition: Attribute table for hydro polygons
    Attribute:
      Attribute_Label: FID
      Attribute_Definition: Internal feature number.
      Attribute_Definition_Source: ESRI
      Attribute_Domain_Values:
        Unrepresentable_Domain: Sequential unique whole numbers that are automatically generated.
    Attribute:
      Attribute_Label: Shape
      Attribute_Definition: Feature geometry.
      Attribute_Definition_Source: ESRI
      Attribute_Domain_Values:
        Unrepresentable_Domain: Coordinates defining the features.
    Attribute:
      Attribute_Label: AREA
      Attribute_Definition: Area of polygon
    Attribute:
      Attribute_Label: PERIMETER
      Attribute_Definition: Polygon perimeter
    Attribute:
      Attribute_Label: HYDRO_P_
      Attribute_Definition: polygon ID
    Attribute:
      Attribute_Label: HYDRO_P_ID
      Attribute_Definition: User ID for polygon
    Attribute:
      Attribute_Label: HYTYPE
      Attribute_Definition: Code to differentiate between land and water masses such as island
      Attribute_Domain_Values:
        Enumerated_Domain:
          Enumerated_Domain_Value: 0
          Enumerated_Domain_Value_Definition: Land Polygon
        Enumerated_Domain:
          Enumerated_Domain_Value: 1
          Enumerated_Domain_Value_Definition: Water Polygon
    Attribute:
      Attribute_Label: SOURCE_NAM
      Attribute_Definition: Code identifying the organization generating the data record.  All data originally created by ADR in 1993 should have an ADR code.
      Attribute_Domain_Values:
        Enumerated_Domain:
          Enumerated_Domain_Value: ADR
          Enumerated_Domain_Value_Definition: Aerial Data Reduction, Inc.
        Enumerated_Domain:
          Enumerated_Domain_Value: ATS
          Enumerated_Domain_Value_Definition: Advanced Tech. Solutions, Inc.
        Enumerated_Domain:
          Enumerated_Domain_Value: LCG
          Enumerated_Domain_Value_Definition: Lancaster County GIS Dept.
    Attribute:
      Attribute_Label: UPD_NAME
      Attribute_Definition: Can be blank, but must be filled in with "ADR" if UPD-DATE, UPD-FEATURE or UPD-ACTION have a value.  A code identifying the organization updating the data record.  All data updated by ADR as part of this contract should have an ADR code.  The first three characters is a code for the organization as listed below.  Characters 4 through 15 should contain an identification code for the employee updating the feature.  Valid ADR codes will be ADR_305 and ADR_319
      Attribute_Domain_Values:
        Enumerated_Domain:
          Enumerated_Domain_Value: ADR
          Enumerated_Domain_Value_Definition: Aerial Data Reduction, Inc.
        Enumerated_Domain:
          Enumerated_Domain_Value: ATS
          Enumerated_Domain_Value_Definition: Advanced Tech. Solutions, Inc.
        Enumerated_Domain:
          Enumerated_Domain_Value: LCG
          Enumerated_Domain_Value_Definition: Lancaster County GIS Dept.
    Attribute:
      Attribute_Label: SOURCE_DAT
      Attribute_Definition: YYYYMMDD format.  Modifies the SOURCE-NAME item, and reflects the date of aerial photography (1988)
    Attribute:
      Attribute_Label: UPD_DATE
      Attribute_Definition: YYYYMMDD format.  Modifies the UPD-NAME item, and reflects the date the data was updated.  Date on which record was last updated in ArcInfo
    Attribute:
      Attribute_Label: SOURCE_MAP
      Attribute_Definition: Identifies the map source (if any) for the record
    Attribute:
      Attribute_Label: UPD_MAP
      Attribute_Definition: Identifies the map source of the update (if any) for the record
    Attribute:
      Attribute_Label: SOURCE_MET
      Attribute_Definition: Identifies the data collection method used to acquire the record.  Encoded with values representing various data collection methods.
      Attribute_Domain_Values:
        Enumerated_Domain:
          Enumerated_Domain_Value: DIG
          Enumerated_Domain_Value_Definition: map digitization
        Enumerated_Domain:
          Enumerated_Domain_Value: PAP
          Enumerated_Domain_Value_Definition: Photogrammetric analysis of aerial photography
        Enumerated_Domain:
          Enumerated_Domain_Value: PSI
          Enumerated_Domain_Value_Definition: Photogrammetric analysis of satellite imagery
        Enumerated_Domain:
          Enumerated_Domain_Value: FR
          Enumerated_Domain_Value_Definition: field reconnaissance
        Enumerated_Domain:
          Enumerated_Domain_Value: GPS
          Enumerated_Domain_Value_Definition: Global Positioning System
        Enumerated_Domain:
          Enumerated_Domain_Value: SCA
          Enumerated_Domain_Value_Definition: Scanning
        Enumerated_Domain:
          Enumerated_Domain_Value: OTH
          Enumerated_Domain_Value_Definition: Other
    Attribute:
      Attribute_Label: UPD_FEATUR
      Attribute_Definition: Identifies the type of feature updated.
      Attribute_Domain_Values:
        Enumerated_Domain:
          Enumerated_Domain_Value: A
          Enumerated_Domain_Value_Definition: arc
        Enumerated_Domain:
          Enumerated_Domain_Value: P
          Enumerated_Domain_Value_Definition: polygon
        Enumerated_Domain:
          Enumerated_Domain_Value: M
          Enumerated_Domain_Value_Definition: point (marker)
        Enumerated_Domain:
          Enumerated_Domain_Value: N
          Enumerated_Domain_Value_Definition: node
        Enumerated_Domain:
          Enumerated_Domain_Value: L
          Enumerated_Domain_Value_Definition: label
        Enumerated_Domain:
          Enumerated_Domain_Value: T
          Enumerated_Domain_Value_Definition: tile
        Enumerated_Domain:
          Enumerated_Domain_Value: C
          Enumerated_Domain_Value_Definition: annotation (character)
        Enumerated_Domain:
          Enumerated_Domain_Value: R
          Enumerated_Domain_Value_Definition: region
        Enumerated_Domain:
          Enumerated_Domain_Value: O
          Enumerated_Domain_Value_Definition: other
    Attribute:
      Attribute_Label: UPD_ACTION
      Attribute_Definition: Identifies the type of update action performed
      Attribute_Domain_Values:
        Enumerated_Domain:
          Enumerated_Domain_Value: A
          Enumerated_Domain_Value_Definition: Add (new feature added)
        Enumerated_Domain:
          Enumerated_Domain_Value: U
          Enumerated_Domain_Value_Definition: update (modification of existing feature shape)
        Enumerated_Domain:
          Enumerated_Domain_Value: M
          Enumerated_Domain_Value_Definition: move (location change for a feature)
        Enumerated_Domain:
          Enumerated_Domain_Value: G
          Enumerated_Domain_Value_Definition: generalize
        Enumerated_Domain:
          Enumerated_Domain_Value: S
          Enumerated_Domain_Value_Definition: split
        Enumerated_Domain:
          Enumerated_Domain_Value: J
          Enumerated_Domain_Value_Definition: unsplit (join)
        Enumerated_Domain:
          Enumerated_Domain_Value: L
          Enumerated_Domain_Value_Definition: spline
        Enumerated_Domain:
          Enumerated_Domain_Value: O
          Enumerated_Domain_Value_Definition: other
    Attribute:
      Attribute_Label: FLAG
    Attribute:
      Attribute_Label: HYNAME
      Attribute_Definition: Name of the drainage polygon feature
Distribution_Information:
  Distributor:
    Contact_Information:
      Contact_Organization_Primary:
        Contact_Organization: Pennsylvania Spatial Data Access (PASDA)
      Contact_Address:
        Address_Type: mailing address
        Address: Land and Water Building
        City: University Park
        State_or_Province: PA
        Postal_Code: 16802
        Country: USA
      Contact_Electronic_Mail_Address: pasda@psu.edu
  Distribution_Liability: The USER shall indemnify, save harmless, and, if requested, defend those parties involved with the development and distribution of this data, their officers, agents, and employees from and against any suits, claims, or actions for injury, death, or property damage arising out of the use of or any defect in the FILES or any accompanying documentation. Those parties involved with the development and distribution excluded any and all implied warranties, including warranties or merchantability and fitness for a particular purpose and makes no warranty or representation, either express or implied, with respect to the FILES or accompanying documentation, including its quality, performance, merchantability, or fitness for a particular purpose. The FILES and documentation are provided "as is" and the USER assumes the entire risk as to its quality and performance. Those parties involved with the development and distribution of this data will not be liable for any direct, indirect, special, incidental, or consequential damages arising out of the use or inability to use the FILES or any accompanying documentation.
  Standard_Order_Process:
    Digital_Form:
      Digital_Transfer_Information:
        Format_Name: ESRI Shapefile
        File_Decompression_Technique: zip
      Digital_Transfer_Option:
        Online_Option:
          Computer_Contact_Information:
            Network_Address:
              Network_Resource_Name: http://pasdadev.erri.psu.edu/lanc/lancdownload2.cgi/lancco_hydro_p
Distribution_Information:
  Distributor:
    Contact_Information:
      Contact_Person_Primary:
        Contact_Person: Steve Gochenaur
        Contact_Organization: Lancaster County GIS Department
      Contact_Address:
        Address_Type: mailing and physical address
        Address: 50 North Duke St., PO Box 83480
        City: Lancaster
        State_or_Province: PA
        Postal_Code: 17608-3480
      Contact_Voice_Telephone: 717-391-7550
      Contact_Electronic_Mail_Address: gochenas@co.lancaster.pa.us
  Distribution_Liability: Not for commercial use or resale. The User shall save Lancaster County, the Commonwealth and the Pennsylvania State University harmless from any suits, claims or actions arising out of the use of the data files or accompanying documentation, or arising out of any defect in the data files or accompanying documentation. Lancaster County, the Commonwealth and the Pennsylvania State University excludes any and all implied warranties and makes no warranty or representation with respect to the data files or accompanying documentation, including quality, performance, merchantability, or fitness for a particular purpose. These data files and documentation are provided AS IS and the User assumes the entire risk as to their quality and performance.
  Standard_Order_Process:
    Digital_Form:
      Digital_Transfer_Information:
        Format_Name: ARC/INFO Export
        Format_Version_Number: 7.2.1
        Transfer_Size: 17.207
      Digital_Transfer_Option:
        Offline_Option:
          Offline_Media: CD-ROM
          Recording_Capacity:
            Recording_Density: 650
            Recording_Density_Units: MB
          Recording_Format: ISO 9660
      Digital_Transfer_Option:
        Offline_Option:
          Offline_Media: 3-1/2 inch floppy disk
          Recording_Capacity:
            Recording_Density: 1.44
            Recording_Density_Units: MB
          Recording_Format: PC
    Digital_Form:
      Digital_Transfer_Information:
        Format_Name: Arcview Shapefile
        Format_Version_Number: 3.1
        Transfer_Size: 17.207
      Digital_Transfer_Option:
        Offline_Option:
          Offline_Media: CD-ROM
    Digital_Form:
      Digital_Transfer_Information:
        Format_Name: DXF
        Transfer_Size: 17.207
    Fees: $25 for premastered CD containing shapefiles.  Custom requests for small area DXF files available for $40/hour processing fee, $10/CD or $1/floppy media charge.
    Ordering_Instructions: Complete instructions and forms available from http://www.co.lancaster.pa.us/GIS.htm
  Standard_Order_Process:
    Non-digital_Form: Hard copy maps can be ordered and created  from Lancaster County GIS
    Digital_Form:
      Digital_Transfer_Information:
        Transfer_Size: 17.207
    Fees:
      8 1/2" x 11" - $5
      11" x 17" - $25

      Standard map 33 1/2" x 45" - $75;  discount rate $50
      Mylar map 33 1/2" x 45" - $100;  discount rate $75

      Custom maps available at a charge of $40/hr.

      Copies of existing maps $25.00
    Ordering_Instructions: Acquire, complete and return Map Request form available at: http://www.co.lancaster.pa.us/GISforms.htm
  Custom_Order_Process: Complete instructions and forms available from http://www.co.lancaster.pa.us/GIS.htm
Metadata_Reference_Information:
  Metadata_Date: 20020107
  Metadata_Review_Date:
  Metadata_Future_Review_Date:
  Metadata_Contact:
    Contact_Information:
      Contact_Person_Primary:
        Contact_Person: Linda McCawley
        Contact_Organization: Lancaster County GIS Department
      Contact_Address:
        Address_Type: mailing and physical address
        Address: 50 North Duke St., PO Box 83480
        City: Lancaster
        State_or_Province: PA
        Postal_Code: 17608-3480
      Contact_Voice_Telephone: 717-391-7550
      Contact_Electronic_Mail_Address: mccawlel@co.lancaster.pa.us
  Metadata_Standard_Name: FGDC Content Standards for Digital Geospatial Metadata
  Metadata_Standard_Version: FGDC-STD-001-1998
  Metadata_Time_Convention: local time
  Profile_Name: ESRI Metadata Profile
